**Integration Manual**

**For**

**Damping Firewall**

**VERSION: 1.0**

**DATE: 15-JAN-2015**

**Prepared By:**

**Spandana Balani**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Rev #** | **Change Description** | **Date** | **Author** |
| 1 | Initial version | 15-Jan-15 | SB |

**Table of Contents**

[1 Abbrevations And Acronyms 4](#_Toc389222316)

[2 References 5](#_Toc389222317)

[3 Dependencies 6](#_Toc389222318)

[3.1 SWCs 6](#_Toc389222319)

[3.2 Global Functions(Non RTE) to be provided to Integration Project 6](#_Toc389222320)

[4 Configuration REQUIREMeNTS 7](#_Toc389222321)

[4.1 Build Time Config 7](#_Toc389222322)

[4.2 Configuration Files to be provided by Integration Project 7](#_Toc389222323)

[4.3 Da Vinci Parameter Configuration Changes 7](#_Toc389222324)

[4.4 DaVinci Interrupt Configuration Changes 7](#_Toc389222325)

[4.5 Manual Configuration Changes 7](#_Toc389222326)

[5 Integration DATAFLOW REQUIREMENTS 8](#_Toc389222327)

[5.1 Required Global Data Inputs 8](#_Toc389222328)

[5.2 Required Global Data Outputs 8](#_Toc389222329)

[5.3 Specific Include Path present 8](#_Toc389222330)

[6 Runnable Scheduling 9](#_Toc389222331)

[7 Memory Map REQUIREMENTS 10](#_Toc389222332)

[7.1 Mapping 10](#_Toc389222333)

[7.2 Usage 10](#_Toc389222334)

[7.3 Non RTE NvM Blocks 10](#_Toc389222335)

[7.4 RTE NvM Blocks 10](#_Toc389222336)

[8 Compiler Settings 11](#_Toc389222337)

[8.1 Preprocessor MACRO 11](#_Toc389222338)

[8.2 Optimization Settings 11](#_Toc389222339)

[9 Appendix 12](#_Toc389222340)

# Abbrevations And Acronyms

|  |  |
| --- | --- |
| **Abbreviation** | **Description** |
| DFD | Design functional diagram |
| MDD | Module design Document |
|  | <ADD more to the table if applicable> |
|  |  |
|  |  |

# References

This section lists the title & version of all the documents that are referred for development of this document

|  |  |  |
| --- | --- | --- |
| **Sr. No.** | **Title** | **Version** |
| 1 | SF35 Damping Firewall | 011 |

# Dependencies

## SWCs

|  |  |
| --- | --- |
| **Module** | **Required Feature** |
| **None** | <Addition of global data, function>\*. |

Note : Referencing the external components should be avoided in most cases. Only in unavoidable circumstance external components should be referred. Developer should track the references.

## Global Functions(Non RTE) to be provided to Integration Project

None

# Configuration REQUIREMeNTS

## Build Time Config

|  |  |  |
| --- | --- | --- |
| **Modules** | **Notes** |  |
| **None** |  |  |

## Configuration Files to be provided by Integration Project

Ap\_DampingFirewall\_Cfg.h for checkpoint enable

## Da Vinci Parameter Configuration Changes

|  |  |  |
| --- | --- | --- |
| **Parameter** | **Notes** | **SWC** |
| **DampingFirewallGeneral**/**DampingFirewallCPEnable** | To enable checkpoints | DampingFirewall |

## DaVinci Interrupt Configuration Changes

|  |  |  |  |
| --- | --- | --- | --- |
| **ISR Name** | **VIM #** | **Priority Dependency** | **Notes** |
| **None** |  |  |  |

## Manual Configuration Changes

|  |  |  |
| --- | --- | --- |
| **Constant** | **Notes** | **SWC** |
| **None** |  |  |

# Integration DATAFLOW REQUIREMENTS

## Required Global Data Inputs

AsstFirewallActive\_Uls\_f32

DampingCmd\_MtrNm\_f32

HwTorque\_HwNm\_f32

InertiaComp\_MtrNm\_f32

MtrVelCRF\_MtrRadpS\_f32

VehicleSpeed\_Kph\_f32

VehicleLonAccel\_KphpS\_f32

BaseAssistCmd\_MtrNm\_f32

WIRCmdAmpBlnd\_MtrNm\_f32

FreqDepDmpSrlComSvcDft\_Cnt\_lgc

Defeat\_Damping\_Svc\_Cnt\_lgc

MEC\_Counter\_Cnt\_enum

## Required Global Data Outputs

CombinedDamping\_MtrNm\_f32

## Specific Include Path present

No

# Runnable Scheduling

This section specifies the required runnable scheduling.

|  |  |  |
| --- | --- | --- |
| **Init** | **Scheduling Requirements** | **Trigger** |
| **DampingFirewall\_Init** |  | On Rte\_Init |

|  |  |  |
| --- | --- | --- |
| **Runnable** | **Scheduling Requirements** | **Trigger** |
| **DampingFirewall\_Per1** | triggered on TimingEvent  Disabled in WARMINIT and OFF | 2ms |

**.**

# Memory Map REQUIREMENTS

## Mapping

|  |  |  |
| --- | --- | --- |
| Memory Section | Contents | Notes |
| DAMPINGFIREWALL\_START\_SEC\_VAR\_CLEARED\_32 |  |  |
| DAMPINGFIREWALL\_START\_SEC\_VAR\_CLEARED\_UNSPECIFIED |  |  |
| DAMPINGFIREWALL\_START\_SEC\_VAR\_CLEARED\_BOOLEAN |  |  |
| DAMPINGFIREWALL\_START\_SEC\_VAR\_CLEARED\_16 |  |  |

\* Each …START\_SEC… constant is terminated by a …STOP\_SEC… constant as specified in the AUTOSAR Memory Mapping requirements.

## Usage

|  |  |  |
| --- | --- | --- |
| **Feature** | **RAM** | **ROM** |
| **None** |  |  |

Table 1: ARM Cortex R4 Memory Usage

## Non RTE NvM Blocks

|  |
| --- |
| **Block Name** |
| **None** |

Note : Size of the NVM block if configured in developer

## RTE NvM Blocks

|  |
| --- |
| **Block Name** |
| **None** |

Note : Size of the NVM block if configured in developer

# Compiler Settings

## Preprocessor MACRO

None

## Optimization Settings

None

# Appendix

*<This section is for appendix>*